{"text_format":"2","workbook":"xlsx","n_sheets":1,"sheets":["Sheet1"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":0,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"Sheet1","index":0,"n_rows":7,"n_cols":10,"rows_kept":7,"cut":false,"hidden":false,"merged":[]}
[null,"首要参考文件","补充参考文件（重复出现的标准以首要参考文件为主，首要参考文件里面没有的参数参考补充参考文件）","气液比正常范围","气液比预报警规则","气液比报警天数","零压报警天数","后处理报警天数","P/V阀预报警","P/V阀临界状态"]
["北京","DB11 208-2019 加油站油气排放控制和限值.pdf","加油站油气回收在线监控设备技术要求和安装指南20180112.pdf","0.85~1.35","在24 h（自然日）内，在线监控系统应监测和保存每次加油的A/L，当每条加油枪有效A/L（每次连续加油量大于15 L）处于表5规定范围的次数达到总次数的25%，在线监控系统应预警，连续5 d出现预警状态应报警，若当日某加油枪加油次数小于5次时，在线监控系统不对该加油枪进行A/L预警和报警判断，并与次日加油次数进行累计，直至大于等于5次后再进行A/L预警和报警判断；在线监控系统应自动关闭A/L报警的加油枪。",5,5,5,"大于正P/V阀开启压力+200Pa，或小于负开启压力-200Pa时预警，超过5分钟报警","油罐压力数据在-1000Pa ~ +600Pa（或-1000Pa~压力/真空阀正开启压力的80%）之外的次数超过总数的25%时，在线监控设备应预警，若连续5天处于预警状态应立即报警"]
["浙江","附录A-加油在线监控设备数据上传协议20190613","加油站油气回收在线监控系统技术指导(2)(1).doc","0.9~1.3","类似北京标准，加油次数小于5次时次日累计",7,7,7,"文档里无该预报警标准参数，按北京标准","文档里无该预报警标准参数，按北京标准"]
["上海","目前不用管","——","——","——","——","——","——"]
["湖南","无，按北京标准","无","按北京标准","按原来标准（不判断加油次数是否小于5，只要气液比超标笔数比例超出25%则预警，达到报警天数则报警）","按北京标准","按北京标准","按北京标准","按北京标准","按北京标准"]
["佛山南海","南海区油气回收在线监测数据管理平台数据上传协议v1.0.1.pdf","他们说是按国标GB20952-2007，但实际他们提供的不一样，而且国标文档应该太旧了，按照他们提供的即可，已总结为《佛山南海预报警规则参数20191216.docx》","0.9-1.3 ","按原来标准",7,7,"不需要","大于正P/V阀开启压力+300Pa，或小于负开启压力-300Pa超过5分钟预警，持续预警7天报警","不需要"]
["山东","山东省生态环境厅关于做好加油站油气回收在线监控工作的通知 (1).pdf",null,"0.9-1.3","按原来标准",7,"无-按北京标准","无-按北京标准","无-按北京标准","无-按北京标准"]