{"text_format":"2","workbook":"xlsx","n_sheets":1,"sheets":["Sheet1"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":0,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"Sheet1","index":0,"n_rows":9,"n_cols":7,"rows_kept":9,"cut":false,"hidden":false,"merged":[]}
["程序/文档名称","版本","是否为新版本","版本改动","是否需要测试","是否已经测试","测试结果说明"]
["油气回收系统安装包V1.14.42.zip","V1.14.42","是","1、修复V1.14.34版本升级后联网运行出错的问题；\n2、增加浙江中石化、山东烟台（云端更换）的联网；\n3、增加配置文件里上传平台2，主平台，是否开启平台2远程传输的配置（需要注意由于配置方式改变，之前浙江地区环保局与浙石油的程序如果升级，“是否开启远程传输”的配置需要重新按照新的配置方法来配置开启）\n4、修复V1.14.36版本配置为浙江中石化开启报警锁枪、液阻非规则报警的问题；","是"]
["油气回收在线监控系统安装配置使用更新文档 V2.0.docx","V2.0","是","1、\t增加配置文件里上传平台2，主平台，是否开启平台2远程传输的配置说明及图片；\n2、\t增加重庆、佛山顺德、浙江中石化的配置说明\n3、\t增加VRC36 串口号的识别与配置简单说明； \n4、\t在油罐配置那里增加传感器配置工具的操作说明；\n5、增加升级前备份的说明","是"]
["加密狗相关问题处理方法 V1.1.docx","V1.1","是","1、增加问题二","是"]
["油气回收在线监控系统数据转移和恢复方法 V1.3.docx","V1.3","是","1、删掉以前的一个数据恢复方法，目前仅保留一个方法；\n2、增加“数据恢复时安装包版本说明”","是"]
["360配置与故障排查方法 V1.1","V1.1","是","1、更新第三点","是"]
["油气回收各地区预报警规则与参数列表 V2.0.xlsx","V2.0","是","1、更换山东烟台的参考文件；\n2、增加佛山顺德地区规则；\n3、增加平台1与平台2的规则区分；\n4、增加浙江浙石油、浙江中石化的规则；\n5、增加液阻报警的上限值（目前只有浙江中石化有）；","可选"]
["部分地区平台的额外配置说明 V2.0","V2.0","是","1、增加浙江中石化配置说明","可选"]
["加油累计不足5笔规则说明 V1.0.docx","V1.0"]