{"text_format":"2","workbook":"xlsx","n_sheets":1,"sheets":["Sheet1"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":0,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"Sheet1","index":0,"n_rows":24,"n_cols":6,"rows_kept":24,"cut":false,"hidden":false,"merged":[[5,1,10,1],[11,1,16,1],[18,0,20,0],[2,0,17,0]]}
[]
["Block","StartAddress(Hex)","Item","Length(Byte)","Description","Input"]
["固件信息","0000 0000","烧录文件主版本号",8,"产品类型（2bytes）\n产品大版本号（2bytes）\n产品小版本号（2bytes）\n修订次数（2bytes）","软件界面输入"]
[null,"0000 0008","烧录文件生成时间",8,"年（1byte）\n月（1byte）\n日（1byte）\n时（1byte）\n分（1byte）\n秒（1byte）","系统时间"]
[null,"0000 0010","烧录文件生成软件所在电脑用户名",32,"该电脑用户名前32个ASCII字符","系统参数"]
[null,"0000 0030","固件A版本号",8,"保留（2bytes）\n产品大版本号（2bytes）\n产品小版本号（2bytes）\n修订次数（2bytes）","固件命名上带有版本信息\n形如：XXXA_01_01_03.bin"]
[null,null,"适配硬件A版本号",8,"部件硬件版本（8bytes）","软件界面输入"]
[null,null,"固件A生成时间",8,"年（1byte）\n月（1byte）\n日（1byte）\n时（1byte）\n分（1byte）\n秒（1byte）","固件文件信息"]
[null,null,"固件A长度",4,"长度(4bytes 小端数据模式)","固件文件信息"]
[null,null,"固件A的CRC16",4,"可执行固件CRC16校验（4bytes 小端数据模式）","软件读取固件文件后生成"]
[null,null,"固件A在文件中的起始地址",4,"地址(4bytes 小端数据模式)","软件规划"]
[null,"0000 0070","固件B版本号",8,"保留（2bytes）\n产品大版本号（2bytes）\n产品小版本号（2bytes）\n修订次数（2bytes）","固件命名上带有版本信息\n形如：XXXB_01_01_03.bin"]
[null,null,"适配硬件B版本号",8,"部件硬件版本（8bytes）","软件界面输入"]
[null,null,"固件B生成时间",8,"年（1byte）\n月（1byte）\n日（1byte）\n时（1byte）\n分（1byte）\n秒（1byte）","固件文件信息"]
[null,null,"固件B长度",4,"长度(4bytes 小端数据模式)","固件文件信息"]
[null,null,"固件B的CRC16",4,"可执行固件CRC16校验（4bytes 小端数据模式）","软件读取固件文件后生成"]
[null,null,"固件B在文件中的起始地址",4,"地址(4bytes 小端数据模式)","软件规划"]
[null,"… …"]
["文件主体","处理后固件A在文件中的起始地址","加密处理后的固件A数据块","固件A长度","小端数据模式"]
[null,"… …"]
[null,"处理后固件B在文件中的起始地址","加密处理后的固件B数据块","固件B长度","小端数据模式"]
[]
[null,"该项可以从软件界面上读取看到"]
[null,"该项必须从软件界面上键入"]