{"text_format":"2","workbook":"xlsx","n_sheets":1,"sheets":["Sheet1"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":0,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"Sheet1","index":0,"n_rows":7,"n_cols":4,"rows_kept":7,"cut":false,"hidden":false,"merged":[]}
["功能模块","在线监控重构方案","科迈捷系统","特点分析/改善考虑"]
["系统架构","后台与油机之间使用TCP/IP通讯。","后台与油机、中继器之间使用lora无线通讯。\n主板可接入更多外界信号如传感器。\n其自身品牌的传感器可以和中继器进行蓝牙连接。","科迈捷在布线、管理其自身品牌传感器等方面有优点"]
["主界面","沿用现有方案，是市场部2023年重新设计的方案","界面较简洁，环境数据只能显示6项，难以满足实际需求","可以考虑是否有需要改善之处"]
["数据查询","油枪预报警统计查询只能从主界面单枪查询。\n可查询最近环保上传信息，交易上传结果可在交易中查询。","可以查询所有油枪的预报警统计和状态。\n可查询所有环保上传记录。","可以增加所有油枪的预报警统计查询。\n可以增加重要数据的上传记录。"]
["报警记录查询","可以在同一界面查询所有传感器的预报警记录。","传感器预报警记录在不同界面查询。可以查询油枪离线记录、低流速记录等。","可以增加油枪离线记录查询与上传至云平台。"]
["系统设置","传感器设置需要使用独立的工具。","传感器等参数都在同个后台系统中配置。","可以把设置工具集成到后台系统。"]
["软件更新","油站人员通过操作界面升级功能进行软件更新","目前并不清楚科迈捷是通过远程访问还是后台连接服务器的方法进行更新"]